

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%   CR et LF    %%%%%%%%%%%%%%%%%%%%%%%%%%
%1 Non-Breaking Spaces
%The most common one is the tilde, ~, that for some reason I like calling a twiddle:
%The following two~words wouldn't be taken away from each other by a line break.

%2 Commands Preventing Automatic Hyphenation
%A word given as argument to the \nobreak command will not be automatically hyphenated, unless it's got a hyphen or you suggested a soft hyphen where to hyphenate it if needs be. However, this command isn't used for keeping words together on a line:
%The following \nobreak{two words} would be taken away from each other by a line break.

%3 Commands Preventing Line Breaks
%Anything given as argument to the \mbox command will be kept together on a line, regardless of their spaces or hyphens.
%The following \mbox{two words} wouldn't be taken away from each other by a line break.
%

%4 Line breaks
%There are three commands here that work the same in the example:
%    \\ (two backslashes)
%    \newline
%    \hfill \break
%

%5 Page breaks
%
%There are two commands to insert page breaks, clearpage and newpage. 



%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%   FONT STYLE  %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%SIZE (Relative to the default document font size)
%Tiny 		Text	{\tiny Text}
%Small 		Text	{\small Text}
%Normal 	Text	{\normalsize Text}
%Large 		Text	{\large Text}
%Huge 		Text	{\huge Text}
%
%STYLE (Note that there are two ways to obtain italic text, where \emph should be preferred over \textit since it’s the command to emphasize text in general. )
%Bold 				Text	\textbf{Text}
%Italic 			Text	\textit{Text}
%Typewriter 		Text	\texttt{Text}
%Sans-Serif 		Text	\ltextsf{Text}
%Serif (Roman) 	Text	\textrm{Text}
%Underline 		Text	\underline{Text}
%
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%  TABLES  %%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%\begin{table}[h!]
%  \begin{center}
%    \caption{Your first table.}
%    \label{tab:table1}
%    \begin{tabular}{l|c|r} % <-- Alignments: 1st column left, 2nd middle and 3rd right, with vertical lines in between
%      \textbf{Value 1} & \textbf{Value 2} & \textbf{Value 3}\\
%      $\alpha$ & $\beta$ & $\gamma$ \\
%      \hline
%      1 & 1110.1 & a\\
%      2 & 10.1 & b\\
%      3 & 23.113231 & c\\
%    \end{tabular}
%  \end{center}
%\end{table}






%Cette première ligne indique la catégorie de chaque question. Le groupe ne doit pas comporter de lettres accentuées !
\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")
  \begin{question}{Ops.1}    
  \bareme{formula=(NBC==NB && NMC==0 ? 1 :  0 )}																

    The picture below is of the oil level on a gear reducer. Is the oil level normal?  
    \newline
  %pour mettre texte des réponses et images dans un "tableau"
    \begin{minipage}[c]{.5\linewidth}            
    
   %\begin{multicols}{2}\AMCBoxedAnswers    
    \begin{reponses}
      \bonne{Yes}
      \mauvaise{No}
    \end{reponses}
    \explain{The oil level must be located between the high (black line) and low (red line) levels.}
  % \end{multicols}
  \end{minipage} \hfill
	\begin{minipage}[c]{.45\linewidth}
	\includegraphics[height=.9\textwidth]{images/oil_level.jpg}
	%\includegraphics[height=3cm]{images/oil_level.jpg}
	\end{minipage} 
	\explain{Good answer 1 Pt, 0 Pt for wrong answer}
  \end{question}
 %%%%%%%%%%%%%%%%%%%%%%%%%%%% LE FAIT de rajouter une question dans le même "élément" fait qu'elles se suivront toujours dans le questionnaire (et ne seront donc pas mélangées et donc découplées) 
    \begin{question}{Ops.2}
    \bareme{formula=(NBC==NB && NMC==0 ? 1 :  0 )}																

    Regarding the Oil level in the previous question, at what level would you consider a safe level for this gear reducer to continue operating?
	\begin{multicols}{2}\AMCBoxedAnswers     
    \begin{reponses}
      \mauvaise{Below the minimum level}
      \mauvaise{Above the "max" line}
      \mauvaise{Below the "min" line}
      \bonne{Between "min" and "max" lines}
    \end{reponses}
    \end{multicols}
    \explain{Good answer 1 Pt, 0 Pt for wrong answer}
  \end{question} 
}




\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")
  \begin{questionmult}{Ops.3}%\bareme{formula=(NBC==NB && NMC==0 ? 2 : NB-NBC + NMC == 1 ? 1 : NB-NBC+NMC==2 ? 0.5 : 0 )}  
\bareme{formula=(NBC==NB && NMC==0 ? 2 : abs(NB-(NBC+NMC))== 1 ? 0.5 :  0 )}																
  
  
    In case of continuously reducing oil level on that machine, what actions can be taken? 
    \newline
  %pour mettre texte des réponses et images dans un "tableau"
    \begin{minipage}[c]{.5\linewidth}            
    
   %\begin{multicols}{2}\AMCBoxedAnswers    
    \begin{reponses}
      \bonne{Communication with control Room}
      \mauvaise{The maintenance will deal with!}
      \bonne{Investigation}
      \mauvaise{Nothing has to be done}
      \bonne{Contain the leak (environment protection)}
      \bonne{Ask for a permit to work}            
    \end{reponses}
    \explain{Even if this is a typical maintenance job, the ops team need to investigate and ask for a PTW}
  % \end{multicols}
  \end{minipage} \hfill
	\begin{minipage}[c]{.45\linewidth}
	\includegraphics[height=.9\textwidth]{images/oil_level.jpg}
	%\includegraphics[height=3cm]{images/oil_level.jpg}
	\end{minipage} 
	\explain{Good answer 2 Pt, 0.5 point for 1 error, 0 Pt for more than 1 error}
  \end{questionmult}
}



\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")
  \begin{question}{Ops.4}
  \bareme{formula=(NBC==NB && NMC==0 ? 0.5 :  0 )}																

  
    In which direction (clockwise/anticlockwise)this pump must turn (tick the correct answer): 
    \newline
  %pour mettre texte des réponses et images dans un "tableau"
    \begin{minipage}[c]{.3\linewidth}            
    
   %\begin{multicols}{2}\AMCBoxedAnswers    
    \begin{reponses}
      \bonne{Anticlockwise}
      \mauvaise{Clockwise}
        
    \end{reponses}
    %\explain{Even if this is a typical maintenance job, the ops team need to investigate and ask for a PTW}
  % \end{multicols}
  \end{minipage} \hfill
	\begin{minipage}[c]{.7\linewidth}
	\includegraphics[height=0.5\textwidth]{images/centrifugal_pump_view.jpg}
	%\includegraphics[height=3cm]{images/oil_level.jpg}
	\end{minipage} 
	\explain{Good answer 0.5 Pt, 0 Pt for wrong answer}
  \end{question}
}



\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")
  \begin{question}{Ops.5}    
  \bareme{formula=(NBC==NB && NMC==0 ? 0.5 :  0 )}																

  
    Is this sludge build-up normal under the belt conveyor? 
    \newline
  %pour mettre texte des réponses et images dans un "tableau"
    \begin{minipage}[c]{.5\linewidth}            
    
   %\begin{multicols}{2}\AMCBoxedAnswers    
    \begin{reponses}
      \bonne{No}
      \mauvaise{Yes}
    \end{reponses}
   
  % \end{multicols}
  \end{minipage} \hfill
	\begin{minipage}[c]{.45\linewidth}
	\includegraphics[height=.7\textwidth]{images/Sludge_under_ash_belt.jpg}
	%\includegraphics[height=3cm]{images/oil_level.jpg}
	\end{minipage}
	\explain{Good answer 0.5 Pt, 0 Pt for wrong answer} 
  \end{question}
 %%%%%%%%%%%%%%%%%%%%%%%%%%%% LE FAIT de rajouter une question dans le même "élément" fait qu'elles se suivront toujours dans le questionnaire (et ne seront donc pas mélangées et donc découplées) 
    \begin{questionmult}{Ops.6}
	\bareme{formula=(NBC==NB && NMC==0 ? 1 : abs(NB-(NBC+NMC))== 1 ? 0.5 :  0 )}																
    
    
    What should we do, if safe to do so (in the case shown in the previous question)?
	\begin{multicols}{2}\AMCBoxedAnswers     
    \begin{reponses}

      \mauvaise{Look at it and pass by}
      \bonne{Adjust the belt conveyor scrappers}
      \bonne{Clean the sludge}
    \end{reponses}
    \end{multicols}
    \explain{Good answer 1 Pt, 0.5 point for 1 error, 0 Pt for more than 1 error}
  \end{questionmult} 
}



\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")
  \begin{questionmult}{Ops.7}
  \bareme{formula=(NBC==NB && NMC==0 ? 1 : abs(NB-(NBC+NMC))== 1 ? 0.5 :  0 )}																

  
    On the drawing below, considering \textbf{valves 2,3 and 4 open}, answer the question:\\
    What is the purpose of line 1? 
    \newline
    \begin{minipage}[c]{.5\linewidth}            
      
    \begin{reponses}
      \bonne{Minimum flow}
      \bonne{Recirculation}
      \mauvaise{Discharge to the process}
    \end{reponses}

  \end{minipage} \hfill
	\begin{minipage}[c]{.45\linewidth}
	\includegraphics[height=.9\textwidth]{images/PID_extract_min_flow.jpg}
	\end{minipage} 
	\explain{Good answer 1 Pt, 0.5 point for 1 error, 0 Pt for more than 1 error}
  \end{questionmult}
}

\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")
  \begin{question}{Ops.8}
  \bareme{formula=(NBC==NB && NMC==0 ? 1 : abs(NB-(NBC+NMC))== 1 ? 0.5 :  0 )}																

  
    On the drawing below, considering \textbf{valves 3 and 4 open and valve 2 closed}, answer the question:\\
    Is there any risk for the installation in this configuration? 
    \newline
    \begin{minipage}[c]{.5\linewidth}            
      
    \begin{reponses}
      \bonne{There is no risk}
      \mauvaise{We will empty the storage tank}
      \mauvaise{The flow is discharged to the process}
    \end{reponses}

  \end{minipage} \hfill
	\begin{minipage}[c]{.45\linewidth}
	\includegraphics[height=.9\textwidth]{images/PID_extract_min_flow.jpg}
	\end{minipage} 
	\explain{Good answer 1 Pt, 0.5 point for 1 error, 0 Pt for more than 1 error}
  \end{question}

  \begin{questionmult}{Ops.9}
  \bareme{formula=(NBC==NB && NMC==0 ? 2 : abs(NB-(NBC+NMC))== 1 ? 0.5 :  0 )}																
 
  
    On the drawing below, considering \textbf{valves 2 and 3 open and valve 4 closed}, answer the question:\\
    Is there any risk for the installation in this configuration? 
    \newline
    \begin{minipage}[c]{.5\linewidth}            
      
    \begin{reponses}
      \bonne{We have a risk of damage on the pump}
      \bonne{There is a risk of pump cavitation}
      \mauvaise{There is no risk}
    \end{reponses}

  \end{minipage} \hfill
	\begin{minipage}[c]{.45\linewidth}
	\includegraphics[height=.9\textwidth]{images/PID_extract_min_flow.jpg}
	\end{minipage} 
	\explain{Good answer 2 Pt, 0.5 point for 1 error, 0 Pt for more than 1 error}
  \end{questionmult}
}





\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")

  \begin{questionmult}{Ops.10}
  \bareme{formula=(NBC==NB && NMC==0 ? 1 : abs(NB-(NBC+NMC))== 1 ? 0.5 :  0 )}																
   
  
    Which type of valve is the one on the picture below?
    \newline
    \begin{minipage}[c]{.55\linewidth}            
      
    \begin{reponses}
      \bonne{A control valve}
      \bonne{It’s possible to manipulate it by hand}
      \mauvaise{A shut-off valve}
      \mauvaise{It’s not possible to manipulate it by hand}
    \end{reponses}

  \end{minipage} \hfill
	\begin{minipage}[c]{.4\linewidth}
	\includegraphics[height=.9\textwidth]{images/control_valve.jpg}
	\end{minipage} 
	\explain{Good answer 1 Pt, 0.5 point for 1 error, 0 Pt for more than 1 error}
  \end{questionmult}
}


\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")

  \begin{question}{Ops.11}
  \bareme{formula=(NBC==NB && NMC==0 ? 0.5 :  0 )}																


  
    Which type of valve is the one on the picture below?
    \newline
    \begin{minipage}[c]{.55\linewidth}            
      
    \begin{reponses}
      \bonne{A safety valve}
      \mauvaise{A shut-off valve}
      \mauvaise{A control valve}
      \mauvaise{A check valve}
    \end{reponses}

  \end{minipage} \hfill
	\begin{minipage}[c]{.4\linewidth}
	\includegraphics[height=.9\textwidth]{images/safety_valve.jpg}
	\end{minipage} 
	\explain{Good answer 0.5 Pt, 0 Pt for wrong answer}
  \end{question}
  
   \begin{question}{Ops.12}
	\bareme{formula=(NBC==NB && NMC==0 ? 0.5 :  0 )}																
   
   
  %\bareme{formula=(NBC==NB && NMC==0 ? 1 : NB-NBC + NMC == 1 ? 0.5 : 0 )}   
      For which purpose the valve in the previous question is it used? 
    \begin{multicols}{2}\AMCBoxedAnswers   
    \begin{reponses}
      \bonne{Eliminate an overpressure}
      \mauvaise{Control the drum water level}
      \mauvaise{Open when the HP steam pressure is too low}
    \end{reponses}
    \explain{Good answer 0.5 Pt, 0 Pt for wrong answer}
    \end{multicols}
 
  \end{question} 
}

\element{Ops}{
%Identifiant de la question, l'id doit être unique (ici c'est "prez")

  \begin{question}{Ops.13}
  \bareme{formula=(NBC==NB && NMC==0 ? 0.5 :  0 )}																
 
  
     Is the cleanliness of the mesh on the phosphate pump filters normal, see picture below?
    \newline
    \begin{minipage}[c]{.55\linewidth}            
      
    \begin{reponses}
      \bonne{No}
      \mauvaise{Yes}
      \mauvaise{Don't konw?}
    \end{reponses}

  \end{minipage} \hfill
	\begin{minipage}[c]{.4\linewidth}
	\includegraphics[height=.7\textwidth]{images/Phosphate_filter_unclean.jpg}
	\end{minipage} 
	\explain{Good answer 0.5 Pt, 0 Pt for wrong answer}
  \end{question}
  
   \begin{question}{Ops.14}
   \bareme{formula=(NBC==NB && NMC==0 ? 0.5 :  0 )}																

   
  %\bareme{formula=(NBC==NB && NMC==0 ? 1 : NB-NBC + NMC == 1 ? 0.5 : 0 )}   
      What should we do with the filter in the previous question?
    %\newline
    \begin{multicols}{2}\AMCBoxedAnswers   
    \begin{reponses}
      \bonne{Clean or replace the filter}
      \mauvaise{Just place it again in the suction part}
      \mauvaise{Remove my gloves to be clean it better}
    \end{reponses}
    \explain{Good answer 0.5 Pt, 0 Pt for wrong answer}
    \end{multicols}
 
  \end{question} 
}












